A close up of a wheel

Description automatically generated

You can see the ripples in the once smooth timing cover, caused by cavitation. These continue to create cavitation.

## Still need some help with this task?

[www.patrolapart.com.au/tutorials](http://www.patrolapart.com.au/tutorials)

You can also contact us via phone if you need but we generally find the video along with this install guide is all you will need!

All of our contact details are listed on the next page.

A picture containing text

Description automatically generated

Contact Us

PATROLAPART/NAVARAPART  
39 Industrial Park Drive  
Lilydale, VIC 3140

Phone:   [(03) 9735 9099](tel:+61%203%209735%209099)  
Email: sales@patrolapart.com.au

LMCT:     10647

Hi-Flow TD42 Water Pump

# 

Installation Guide

A picture containing text

Description automatically generated

In this guide we will show you how to check your impellor-to-timing case clearance while fitting a Hi-Flow water pump. The wrong clearance can cause cavitation which has a large impact on the efficiency of your TD42 cooling system.

## You will need

Just some simple tools for this task!

* Small amount of Blu tack
* 12mm socket
* 14mm socket
* Ratchet or Impact Gun

A close up of an engine

Description automatically generated

### Check your Impellor-to-Timing Case Clearance.

The clearance on these water pumps has been set using a New Genuine Timing Cover, each pump is test fitted after assembly.

With the old water pump pulled off, as pictured above, clean the mating surface back to bare alloy.

### We will run you through a couple of steps to check your Air Gap for your specific engine. All of this is to be done dry, with no extra sealant or adhesive to get it correct before final assembly.

### Method

## Apply a small amount of Blu Tack as pictured below to one of the impellor fins.

A close up of a wheel

Description automatically generated

## Fit the water pump to the timing case, with the gasket installed, and do up firmly. (we suggest using only the three bolts as circled in the picture below for test fitting).

A close up of an engine

Description automatically generated

## Remove the water pump again and inspect the thickness of the Blu Tack left on the impellor fin. We are aiming for an approximate 1mm clearance.

## If you find it is too thick, remove the gasket and try again.

1. If you find the Blu Tack splitting apart or squashed out completely after doing this step, then you don’t have enough gap and need to add a 2nd gasket.

Please use the photo below to compare the thickness required of the Blu Tack.

A picture containing ground, animal, laying, floor

Description automatically generated

Too thin,

Split apart

Perfect,

Very thin

Too thick

Way too thick